Lost data in VX-1 CPU for Squelch & S meter functions
Reprogramming Procedure:
Note: ** in procedure below repsents any number sequence
- Press & hold the VOL + FW + MON buttons down together and power up the radio. 
- The Display should now show HSSQ03 (note: the important 3 is the small 3 at 
  the top of the display. If anything but 3 appears at the top of the display, 
  press the BAND button until the 3 appears)
- Press the UP button to display HASQ** (Auto Squelch Hysteresis)
- Turn the dial until the display shows HASQ08
- Press the UP button to display THSQ** (Squelch Preset Threshold)
- Turn the dial until the display shows THSQ4F
- Press the UP button to display TISQ** (Squelch Preset Tight)
- Turn the dial until the display shows TISQ2F
- Press the UP button 2 times to display S1LV** (S meter S1 level adjust)
- Turn the dial until the display shows S1LV34
- Press the UP button to display S9LV** (S meter S9 level adjust)
- Turn the dial until the display shows S9LVA3
- Press the UP button to display HSSQ03 (Squelch Hysteresis)
- Press the BAND button 3 times until the display shows HSSQ06 (again note: this 
  is the small 6 at the top of the display) 
- Press the UP button to display HASQ**
- Turn the dial until the display shows HASQ08
- Press the UP button to display THSQ**
- Turn the dial until the display shows THSQ4D
- Press the UP button to display TISQ**
- Turn the dial until the display shows TISQ30
- Press the UP button 2 times to display S1LV**
- Turn the dial until the display shows S1LV27
- Press the UP button to display S9LV**
- Turn the dial until the display shows S9LV96
- Press the FW button for 0.5 seconds to store these settings into memory. The 
  radio will return to normal mode. 
- The reprogramming procedure is now complete.
 