*VHF(H)A
1360
1560
*VHF(H)B
1500
1740
*UHF(L)A
4030
4300
*UHF(L)B
4500
4700
*COMM
COM1:
COM2:
*MODEL
VHF(H) A Band
VHF(H) B Band
UHF(L) A Band
UHF(L) B Band
*AUX
Type 1
Type 2
Type 3
*PRI-TIME
0.50 sec
0.75 sec
1.00 sec
1.50 sec
*PRI-CYCLE
1 to 8
1 to 4
*SCAN-HOLD
Open/NSQ     
Busy/NSQ     
Open/Signalng
Busy/Signalng
*HOLDCD
0.3 sec 
2.5 sec 
5.0 sec 
Infinite
*DEL-TABLE
Power/Scan
Power Off 
Scan Off  
No Clear  
*SCAN-TYPE
Normal   
Modified 
Secondary
PS       
Trunking 
*BCLO
NSQ      
Signaling
Special  
Disable  
*POWER
Infinite
20 sec  
10 sec  
5 sec   
*TXTOT
30 sec  
60 sec  
90 sec  
120 sec 
150 sec 
180 sec 
210 sec 
Infinite
*PTT
15 sec
30 sec
45 sec
60 sec
*BEEP-ON
Normal
Long  
*INTER
500 ms
550 ms
600 ms
650 ms
700 ms
750 ms
800 ms
850 ms
*INJ
High Side
Low Side 
*PLL
2.5 
5.0 
6.25
*PLL1
5.0 
6.25
*CH-PWR
Low Only
Normal  
*CH-SIG
None 
DCS  
CTCSS
*CTCSS
 67.0
 71.9
 74.4
 77.0
 79.7
 82.5
 85.4
 88.5
 91.5
 94.8
 97.4
100.0
103.5
107.2
110.9
114.8
118.8
123.0
127.3
131.8
136.5
141.3
146.2
151.4
156.7
162.2
167.9
173.8
179.9
186.2
192.8
203.5
210.7
218.1
225.7
233.6
241.8
250.3
 74.0
 69.3