; File: RCWKeyer_Bands.txt
; This file contains a list of user defined bands and 
;  "frequencies of interest" for the Remote CW Keyer .
; Details in the manual (manual/Remote_CW_Keyer.htm#User_Defined_Bands) !
; After a 'fresh installation', this file is just a TEMPLATE, placed here
; by the self-extracting installer (Remote_CW_Keyer_Setup.exe) .
;
; It may be edited with a plain text editor, to restrict the TX frequencies
; to what your national regulations, tuner, and antenna permits.
;
; If a particular setup does NOT support a certain band (neither RX nor TX),
; comment out the line for that band by inserting a semicolon at the begin.
; Otherwise, if the rig can report its own 'TX band edges' (like modern
; Icom rigs, IC-7300, IC-9700, etc), you can leave those bands in the list
; because the RCW Keyer ignores entries outside the rig's supported
; frequency ranges (at least for transmission).
;
; If a particular band shall be 'receive only', change "tx=1" to "tx=0".
;
; If ALL BANDS are commented out, or RCWKeyer_Bands.txt doesn't exist
; in the folder with the executable, the Remote CW Keyer will use 
; all frequency ranges that *the rig* claims it can transmit on, which is
; usually NOT desired in a truly remote operation !
; For example, an IC-7300 modified to transmit on 60 meters (5.3xx MHz)
; reports being able to transmit from 0.1 to 74.8 MHz, 
; which is dangerous for your TRX and license. Thus the need for THIS FILE.
;
; If you're not in ITU Region 1, double-check the frequency ranges (in MHz).
;
[Bands]  ; section with User Defined Bands :
         ; mo=allowed operating modes  tx=permission to transmit,
         ; df=default frequency        dm=default operating mode,
         ; na="name" (optional, for the band list display)
1.81-2.0      mo=CW,LSB tx=0 df=1.8200 dm=CWN
3.50-3.8      mo=CW,LSB tx=1 df=3.0595 dm=CWN
5.3515-5.3665 mo=CW     tx=1 df=5.3525 dm=CWN na="60 m EU" ; transmit here in DL, WRC-15 band
5.2585-5.2640 mo=CW     tx=0 df=5.2600 dm=CWN na="60 m UK" ; receive-only in DL, TX only in UK
7.00-7.2      mo=CW,LSB tx=1 df=7.030  dm=CWN
10.1-10.13    mo=CW     tx=1 df=10.123 dm=CWN ; CW suggested only between 10.1 and 10.13 MHz
14.0-14.35    mo=CW,USB tx=1 df=14.060 dm=CWN
18.068-18.168 mo=CW,USB tx=1 df=18.090 dm=CWN
21.0-21.45    mo=CW,USB tx=1 df=21.050 dm=CWN
24.89-24.99   mo=CW,USB tx=1 df=24.910 dm=CWN
28.0-29.70    mo=CW,USB tx=1 df=28.050 dm=CWN
50.0-50.4     mo=CW,USB tx=1 df=50.087 dm=CWN ; 50.4 = begin of the "new" beacon band
144.0-144.4   mo=CW,USB tx=1 df=144.05 na="2m NB" dm=CWN
144.4-146.0   mo=ALL    tx=1 df=145.50 na="2m div" dm=FMN
; simplified kind-of "bandplan" (here: for Germany):
430.0-431.9875 mo=FM,DV tx=1 na="70cm FM,Rptr" 
432.0-432.399 mo=CW,USB tx=1 na="70cm NB" df=432.2 dm=USB
432.4-432.49  mo=CW,USB tx=0 na="70cm Bcn"
432.5-439.999 mo=ALL    tx=1 na="70cm Rpt"
1240.0-1243.25 mo=ALL   tx=1 na="23cm Rpt"
1243.25-1260.0 mo=ALL   tx=1 na="23cm ATV"
1260.0-1270.0  mo=ALL   tx=1 na="23cm Sat"
1270.0-1272.0  mo=ALL   tx=1 na="23cm Rpt"
1272.0-1294.0  mo=ALL   tx=1 na="23cm ATV"
1294.0-1296.0  mo=ALL   tx=1 na="23cm Dig"
1296.0-1296.4  mo=CW,USB tx=1 na="23cm NB" df=1296.2 dm=USB
1296.4-1296.7  mo=CW,USB tx=1 na="23cm div"
1296.8-1296.994 mo=CW   tx=0 na="23cm Bcn"
1296.994-1297.981 mo=FM,DV tx=1 na="23cm FM,DV"
1298.0-1300.0  mo=FM,DV tx=1 na="23cm Rptr"

[Frequencies]  ; section with User Defined Frequencies :
    ; Up to three listed PER BAND will appear in the 
    ; multi-column 'Bands' list,
    ; unless the rig itself reported 'band stacking registers'.
    ; If less than 3 frequencies per band are defined below,
    ; or can be read from the modern Icom's transceiver's
    ; "band stacking registers" via CI-V, the band's
    ; "default" frequency ("df=.." from the [Bands] section)
    ; will be appended to the multi-column 'Bands' display.
    ; Note: The NCDXF/IARU International Beacon frequencies
    ;       have been added in EiBi_Frequencies.txt,
    ;       thus no need to specify them HERE.
    ; Basic format: Frequency_in_MHz mode=CW (or CWN, or whatever)
3.505  mo=CWN  na="80m CW DX"
3.560  mo=CWN  na="80m CW QRP"
7.015  mo=CWN  na="40m CW DX" 
7.030  mo=CWN  na="40m CW QRP"
5.3525 mo=CWNN na="60m CW"
10.123 mo=CWN  na="30m CW"
21.060 mo=CWN  na="15m CW QRP"
24.910 mo=CWN  na="12m CW QRP"
28.060 mo=CWN  na="10m CW QRP"
50.090 mo=CWN  na="6m CW CQ"
50.110 mo=CWN  na="6m CQ DX"
144.05 mo=CWN  na="2m CW CQ"
432.05 mo=CWN  na="70cm CW CQ"
432.20 mo=USB  na="70cm SSB CQ"
   



