{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["PLAY","PLAY (2)"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PLAY","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
[null,"USB0::0x0699::0x0401::C001967::0::INSTR"]
[null,"Insert VISA address for the Tek MSO4104 USB port in cell B1 above.  It's possible to get this address using Keysight Connection Expert"]
[null,null,null,null,null,null,"For example, Tek MSO4104 asset A004656 has visa address  USB0::0x0699::0x0401::C001967::0::INSTR"]
[]
["Step 1",null,null,"This checks the USB connection"]
[]
[]
[]
["Step 2"]
[]
[null,null,null,null,null,"39.0000E-9\n"]
[null,null,null,null,null,null,"Sample Counter"]
["Step 3","Set Number of samples",null,null,10,null,10]
[]
[]
["Step 4",null,null,null,null,"38.4667E-9\n"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"This measures the time delay  from CH1 to CH4 for the required number of samples"]
[]
[null,"Data saved to c:\\logger\\logdelay.txt"]
[]
[null,"Press CTRL + PAUSE/BREAK keys to halt the program if required"]

{"sheet":"PLAY (2)","index":1,"n_rows":43,"n_cols":14,"rows_kept":43,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,null,null,"Press CTRL + PAUSE/BREAK keys to halt the program if required"]
[]
[]
["Step 1"]
[]
[]
[]
["Step 2"]
[null,null,null,null,null,"CH4 Delay","CH3 delay"]
[null,null,null,null,null,9.9100000000000005E+37,9.9100000000000005E+37]
[null,null,null,null,null,null,"Sample Counter"]
["Step 3","Set Number of samples",null,null,10,null,10]
[]
[null,"Sample rate defined by 1PPS activity"]
[]
[]
[]
[]
[]
[]
[]
[null,null,"This measures the time delay  from CH1 to CH4 and from CH1 to CH3 for the required number of samples"]
[null,null,"Data saved to c:\\logger\\logdelay.txt"]
[]
[]
[null,null,null,null,null,null,"OVEN"]
["Step 4"]
[null,null,null,null,null,"Set Point",28,"degC"]
[null,null,null,null,null,"Hysteresis",0.1,"degC",null,null,null,"TC CH0  (COLD JUNC)",21,"degC"]
[null,null,null,null,null,null,null,null,null,null,null,"TC CH1",22,"degC"]
[null,null,null,null,null,null,null,null,null,null,null,"TC CH2",31.799999999999983,"degC"]
[null,null,null,null,null,"DUT Temperature",31.799999999999983,"degC"]
[]
[]
[null,"USB0::0x0699::0x0401::C002145::0::INSTR"]
[null,"Insert VISA address for the Tek MSO4104 USB port in cell B36 above.  It's possible to get this address using Keysight Connection Expert"]
[null,null,null,null,null,null,"For example, Tek MSO4104 asset A004656 has visa address  USB0::0x0699::0x0401::C001967::0::INSTR"]
[null,"GPIB0::30::INSTR"]
[null,"InsertGPIB address for the Tti PSU in cell B39 above.  It's possible to get this address using Keysight Connection Expert"]
[]
[null,null,null,null,null,"TRL Scope =","USB0::0x0699::0x0401::C001967::0::INSTR"]
[null,null,null,null,null,"JMR Scope =","USB0::0x0699::0x0401::C002145::0::INSTR"]