{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["ADF5355"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ADF5355","index":0,"n_rows":17,"n_cols":58,"rows_kept":17,"cut":false,"hidden":false,"merged":[[4,8,13,12]]}
["Target Freq",2112,"MHz",null,"Ref Doubler","No",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fundamental","Yes"]
["Ref",122.88,"MHz",null,"Ref Div2","yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Divided","No"]
["Chan Space",0.2,"MHz",null,"Feedback","Fundamental"]
[]
["OutDiv",2,null,null,"Reg0","200220",null,null,"Enter the Target Frequency, Reference clock multiplier/Dividor selections and click the calc button.\n\nN will turn red if outside recommended range; change ref doubler or clock divisor to correct.\n\nMod2 will turn red if over 16383",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,310]
["PFD",122.88,null,null,"Reg1","6000001"]
["N",34.375,null,null,"Reg2","C002"]
["N_Int",34,null,null,"Reg3","3"]
["Frac1",6291456,null,null,"Reg4","3000A784"]
["Frac1 Int",6291456,null,null,"Reg5","800025"]
["Frac2",0,null,null,"Reg6","15220476"]
["Frac2 Int",0,null,null,"Reg7","120000E7"]
["Mod2",3072,null,null,"Reg8","102D0428"]
["GCD",40,null,null,"Reg9","302FCC9"]
["ADCClkDiv",255,null,null,"Reg10","C03FFA"]
[null,null,null,null,"Reg11","61300B"]
[null,null,null,null,"Reg12","1041C"]