fodtrack.conf(5)         LX2GT Sat Tools         fodtrack.conf(5)



NAME
       /etc/fodtrack.conf - Configuration file for fodtrack rotor
       driver

DESCRIPTION
       The fodtrack program uses a configuration file called fod-
       track.conf. This configuration file must be located in the
       /etc directory, and is used to configure the driver.

PARAMETERS
       PARDEV=<device>
              Parallel port device

       MAXAZIMUTH=<angle>
              Maximal angle the hozizontal rotor is able to turn.

       ELEVATIONCORRECTION=<angle>
              Correction applied to the elevation angle

       AZIMUTHCORRECTION=<angle>
              Correction applied to the azimuth angle AZIMUTHCEN-
              TER=<N or S> Sets the rotator azimuth scale  center
              (eg. G5400-B is S)

FILES
       /etc/fodtrack.conf

SEE ALSO
       fodtrack(5)



Luc Langehegermann             0.1               fodtrack.conf(5)
