MHEARD(1)           Linux Programmer's Manual           MHEARD(1)



NAME
       mheard - display AX.25 calls recently heard.

SYNOPSIS
       mheard [-d cmns] [-n] [-o cfpt] [-v] [port...]

DESCRIPTION
       Mheard  displays  information  about  most  recently heard
       AX.25 callsigns, the interface upon which they were heard,
       the  total  packets  heard, the time at which the last one
       was heard and other information.  Mheard displays  differ-
       ent information, in different orders depending on the set-
       tings of the arguments. Information on specific ports  can
       be displayed by giving the port names as arguments.

OPTIONS
       -d cmns      Sets  the  information  that is displayed for
                    each  AX.25  callsign  heard.  The  different
                    arguments are:

                    c    Display  all the information with regard
                         to  callsigns,  from-callsign,  to-call-
                         sign,  port  name,  and  any digipeaters
                         that may be in use.

                    m    Display miscellaneous  information,  the
                         from-callsign,   port  name,  no  frames
                         heard, the last type  of  frames  heard,
                         and which different PIDs have been heard
                         from that station.

                    n    Display the default information. This is
                         the  from-callsign, port name, no frames
                         heard and the date and time last  heard.

                    s    Displays  statistics  about  the station
                         heard, the from-callsign, port name,  no
                         I frames, no S frames, no U frames, time
                         first heard, and time last heard.

       -n           Supress the displaying of titles.

       -o cfpt      Sets the ordering  of  the  information  dis-
                    played.  The  meanings of the different argu-
                    ments are:

                    c    Sort list by from-callsign.

                    f    Sort list by number of frames heard.

                    p    Sort list by port name.

                    t    Sort list by the time last  heard,  this
                         is the default.

       -v           Display the version.

FILES
       /var/ax25/mheard/mheard.dat
       /etc/ax25/axports

SEE ALSO
       ax25(4), mheardd(8).

AUTHOR
       Jonathan Naylor G4KLX <g4klx@g4klx.demon.co.uk>



Linux                     19 August 1996                MHEARD(1)
