# XBee_RX64 Struct Reference
[XBee Packet Types]

An incoming data packet with a 64-bit address. More...

## Data Fields
uint8 | source [8]
| the 64-bit (8-byte) address of the sender.
uint8 | rssi
| the signal strength of the received message.
uint8 | options
| bit 1 is Address Broadcast, bit 2 is PAN broadcast.
uint8 | data [89]
| a buffer containing the value of the incoming packet.

## Detailed Description

An incoming data packet with a 64-bit address.

Definition at line 116 of file xbee.h.

## Field Documentation

uint8 XBee_RX64::data[89]

a buffer containing the value of the incoming packet.

Definition at line 121 of file xbee.h.

uint8 XBee_RX64::options

bit 1 is Address Broadcast, bit 2 is PAN broadcast.

Other bits reserved.

Definition at line 120 of file xbee.h.

uint8 XBee_RX64::rssi

the signal strength of the received message.

Definition at line 119 of file xbee.h.

uint8 XBee_RX64::source[8]

the 64-bit (8-byte) address of the sender.

Definition at line 118 of file xbee.h.