# XBee_ATCommandResponse Struct Reference
[XBee Packet Types]

The structure used for a response to a standard AT Command packet. More...

## Data Fields
uint8 | frameID
| the ID that this response is referring to.
uint8 | command [2]
| the 2-character AT command.
uint8 | status
| response value - 0 (OK) or 1 (ERROR).
uint8 | value [96]
| a buffer containing the value of the AT command response.

## Detailed Description

The structure used for a response to a standard AT Command packet.

Definition at line 70 of file xbee.h.

## Field Documentation

uint8 XBee_ATCommandResponse::command[2]

the 2-character AT command.

Definition at line 73 of file xbee.h.

uint8 XBee_ATCommandResponse::frameID

the ID that this response is referring to.

Definition at line 72 of file xbee.h.

uint8 XBee_ATCommandResponse::status

response value - 0 (OK) or 1 (ERROR).

Definition at line 74 of file xbee.h.

uint8 XBee_ATCommandResponse::value[96]

a buffer containing the value of the AT command response.

Definition at line 75 of file xbee.h.