# XBee_TX16 Struct Reference
[XBee Packet Types]

The structure used to transmit a data packet with a 16-bit destination address. More...

## Data Fields
uint8 | frameID
| the ID for this packet that subsequent response/status messages can refer to.
uint8 | destination [2]
| the 16-bit (2-byte) address of the destination.
uint8 | options
| 0x01 (disable ACK) or 0x04 (Send with Broadcast PAN ID).
uint8 | data [96]
| a buffer containing the value of the outgoing packet.

## Detailed Description

The structure used to transmit a data packet with a 16-bit destination address.

Definition at line 92 of file xbee.h.

## Field Documentation

uint8 XBee_TX16::data[96]

a buffer containing the value of the outgoing packet.

Definition at line 97 of file xbee.h.

uint8 XBee_TX16::destination[2]

the 16-bit (2-byte) address of the destination.

Definition at line 95 of file xbee.h.

uint8 XBee_TX16::frameID

the ID for this packet that subsequent response/status messages can refer to.

Definition at line 94 of file xbee.h.

uint8 XBee_TX16::options

0x01 (disable ACK) or 0x04 (Send with Broadcast PAN ID).

Definition at line 96 of file xbee.h.