# XBee_RX16 Struct Reference
[XBee Packet Types]

An incoming data packet with a 16-bit address. More...

## Data Fields
uint8 | source [2]
| the 16-bit (2-byte) address of the sender.
uint8 | rssi
| the signal strength of the received message.
uint8 | options
| bit 1 is Address Broadcast, bit 2 is PAN broadcast.
uint8 | data [95]
| a buffer containing the value of the incoming packet.

## Detailed Description

An incoming data packet with a 16-bit address.

Definition at line 127 of file xbee.h.

## Field Documentation

uint8 XBee_RX16::data[95]

a buffer containing the value of the incoming packet.

Definition at line 132 of file xbee.h.

uint8 XBee_RX16::options

bit 1 is Address Broadcast, bit 2 is PAN broadcast.

Other bits reserved.

Definition at line 131 of file xbee.h.

uint8 XBee_RX16::rssi

the signal strength of the received message.

Definition at line 130 of file xbee.h.

uint8 XBee_RX16::source[2]

the 16-bit (2-byte) address of the sender.

Definition at line 129 of file xbee.h.