# XBee_TXStatus Struct Reference
[XBee Packet Types]

When a transmit request is completed, the module sends a transmit status message. More...

## Data Fields
uint8 | frameID
| the ID that this response is referring to.
uint8 | status
| can have values of: 0 - success 1 - No ACK received 2 - CCA failure 3 - Purged.

## Detailed Description

When a transmit request is completed, the module sends a transmit status message.

Definition at line 103 of file xbee.h.

## Field Documentation

uint8 XBee_TXStatus::frameID

the ID that this response is referring to.

Definition at line 105 of file xbee.h.

uint8 XBee_TXStatus::status

can have values of:

- 0 - success
- 1 - No ACK received
- 2 - CCA failure
- 3 - Purged.

Definition at line 106 of file xbee.h.