# XBee_TX64 Struct Reference
[XBee Packet Types]

The structure used to transmit a data packet with a 64-bit destination address. More...

## Data Fields
uint8 | frameID
| the ID for this packet that subsequent response/status messages can refer to.
uint8 | destination [8]
| the 64-bit (8-byte) address of the destination.
uint8 | options
| 0x01 (disable ACK) or 0x04 (Send with Broadcast PAN ID).
uint8 | data [90]
| a buffer containing the value of the outgoing packet.

## Detailed Description

The structure used to transmit a data packet with a 64-bit destination address.

Definition at line 81 of file xbee.h.

## Field Documentation

uint8 XBee_TX64::data[90]

a buffer containing the value of the outgoing packet.

Definition at line 86 of file xbee.h.

uint8 XBee_TX64::destination[8]

the 64-bit (8-byte) address of the destination.

Definition at line 84 of file xbee.h.

uint8 XBee_TX64::frameID

the ID for this packet that subsequent response/status messages can refer to.

Definition at line 83 of file xbee.h.

uint8 XBee_TX64::options

0x01 (disable ACK) or 0x04 (Send with Broadcast PAN ID).

Definition at line 85 of file xbee.h.