# XBee_IO64 Struct Reference
[XBee Packet Types]

An incoming packet with IO data from a 64-bit address. More...

## Data Fields
uint8 | source [8]
| the 64-bit (8-byte) address of the sender.
uint8 | rssi
| the signal strength of the received message.
uint8 | options
| bit 1 is Address Broadcast, bit 2 is PAN broadcast.
uint8 | samples
| the number of samples in this packet.
uint8 | channelIndicators [2]
| bit mask indicating which channels have been sampled.
uint8 | data [86]
| a buffer containing the IO values as indicated by channelIndicators.

## Detailed Description

An incoming packet with IO data from a 64-bit address.

Definition at line 138 of file xbee.h.

## Field Documentation

uint8 XBee_IO64::channelIndicators[2]

bit mask indicating which channels have been sampled.

Definition at line 144 of file xbee.h.

uint8 XBee_IO64::data[86]

a buffer containing the IO values as indicated by channelIndicators.

Definition at line 145 of file xbee.h.

uint8 XBee_IO64::options

bit 1 is Address Broadcast, bit 2 is PAN broadcast.

Other bits reserved.

Definition at line 142 of file xbee.h.

uint8 XBee_IO64::rssi

the signal strength of the received message.

Definition at line 141 of file xbee.h.

uint8 XBee_IO64::samples

the number of samples in this packet.

Definition at line 143 of file xbee.h.

uint8 XBee_IO64::source[8]

the 64-bit (8-byte) address of the sender.

Definition at line 140 of file xbee.h.