# XBee_ATCommand Struct Reference
[XBee Packet Types]

The structure used for a standard AT Command packet. More...

## Data Fields
uint8 | frameID
| the ID for this packet that subsequent response/status messages can refer to.
uint8 | command [2]
| the 2-character AT command.
uint8 | parameters [97]
| a buffer that holds the value of the AT command.

## Detailed Description

The structure used for a standard AT Command packet.

Definition at line 60 of file xbee.h.

## Field Documentation

uint8 XBee_ATCommand::command[2]

the 2-character AT command.

Definition at line 63 of file xbee.h.

uint8 XBee_ATCommand::frameID

the ID for this packet that subsequent response/status messages can refer to.

Definition at line 62 of file xbee.h.

uint8 XBee_ATCommand::parameters[97]

a buffer that holds the value of the AT command.

Definition at line 64 of file xbee.h.