Hi, 
 This is a resend with correction. i.e., the logical choice is "A", NOT
"B" as I incorrectly stated. So I have resent again My apologies.

 

> 
> From: YU7RD @ 9A0BBS.HRV.EU (Vlado)
> To:   ALL @ WW
> Reply-To: YU7RD @ 9A0YDA.HRV.EU
> X-Info: No login password
> 
> Hi everybody, I wont to know ordering the pinouts on USB port (4-pins).
> Please tell me something about it, what is +5V, gnd and others...
> Thanks in advance and all the


Hi, 
 Looking at a manual I have handy for a BioStar 8500TVX motherboard, 
it has listings for 2 USB ports
     These are as written:
	Pin A1: VCC		Pin B1: VCC
	Pin A2: PortO DATA-	Pin B2: Port1 DATA-
	Pin A3: Port0 DATA+	Pin B3: Port1 DATA+
	Pin A4: GND		Pin B4: GND

For a MictoStar board (MS5184) which has 10 pins 

	1 (..)
	  (..)
	  (..)
	  (..)
	  (..)

	Pin 1: VCC (+5v)	Pin 6: GND
	Pin 2: PortO DATA-	Pin 7: GND
	Pin 3: Port0 DATA+	Pin 8: Port1 DATA+
	Pin 4: GND		Pin 9: Port1 DATA-
	Pin 5: GND		Pin 10:Vcc (+5v)

	Unfortunately, the pin numbering sequence is not defined, so some
checking of the board will need to be done. Maybe someone will be able to
clarify if it is "A" or "B". (logically it would appear to be "B".)

 	   A			   B

        1 (..) 10		1 (..) 6
	  (..)                    (..)
	  (..)          	  (..)
	  (..)			  (..)	
	5 (..)  6               5 (..) 10

  Anyway, I hope this will help,

73 de Allen, ZL1UIC @ ZL1UX
        Cambridge, N.Z.,      RF72RC

	Message timed: 09:50 on 19 Jun 03
	Message sent using WinPack-AGW V6.80



73 de Allen, ZL1UIC @ ZL1UX
        Cambridge, N.Z.,      RF72RC

	Message re-timed: 14:37 on 19 Jun 03
	Message re-sent using WinPack-AGW V6.80


     
Using p166, W98se, AGW-PE, Baycom modem, IC-2A, Digitor 30w amp.

