These are text commands that can be entered from the keyboard
\callsign [callsign]
	Sets your callsign to the following string.
\grid [grid]
	Sets your grid (six letters) that is used in FT8 and other modes to 
	indicate your approximate locationi.
\freq [frequency in Hz or Kilohertz]
	You can also type just 'f' instead 'freq' 
	if you the type '\f 7050' it will set be the same as '\freq 7050000'
\cwdelay [100-2000] msec. How long radio remains in transmit in CW before
	timing out to rx. ex: "\cwdelay 500"
\cwinput [key\keyer\kbd]
	Chooses the CW input method between straight key(key), Iambic keyer(keyer)
	and the keyboard (kbd).
\mode [USB\LSB\etc..]...
	Chooses from the modes available in the mode selection control.
	You can use 'm' instead of 'mode'
\t 
	Puts the radio into transmit. You can also use Ctrl-T
\r 
	Puts the radio into receive. You can also use Ctrl-R
\topen [server]:[port]
	Opens a telnet session with an RBN or a DX cluster telnet server.
	It works with ip address as well as domain names
	Ex: \topen dxc.g3lrs.org.ul:7300
\tclose 
	Closes the existing telnet session
\w [telnet command string]
	Writes the remaining text (skipping the space after '\w') to the
	currently opened telnet server
\txpitch [in Hz]
	Sets the tone of transmit tone of the CW. 
	Ex: \txpitch 700
\

	
	



