**Following two are for the version of 10.000 contacts**

**Retevis RT82 (GPS-REC)-S** **4.15.bin for GPS version**

**Retevis RT82 (REC)-D** **4.15.bin for common version**

**Following two are for the version of 100.000 contacts**

**Retevis RT82 (CSV-GPS)-P** **4.15.bin for GPS version**

**Retevis RT82 (CSV)-V** **4.15.bin for common version**

**Firmware version: 4.05**

**Programming software: V1.22**

**Update content:**

1. Add the function VFO locked
2. Add the special frequency band: 150-160mhz and 450-460mhz
3. Add the Switching function between VFO locked,normal frequency band and special frequency band

**How to  switch?**  
Press the top two side-keys to turn on  your radio, It will come the options for you to choose.