[PROFILE]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Advice          Yes             The advisor popups
Age             -none-          Used for JART contest
AutoCr          58              The column that the onscreen rtty wraps
AutoReindex     Yes             Rebuilds index file everytime, leave it on!
AutoRescore     True            The score is recalculated as each qso is logged
Call            -none-          Your callsign
City            -none-          Your city/town/etc
Class           Single Op       Your classification
Club            -none-          Your contest club
CqZone          -none-          Your CQ Zone 01-40
DataCount       40              If recording data, data count for each write
DateMask        yymmdd          Choices: yymmdd, mmddyy, or ddmmyy
Detector        1               1=old way, 2=new alternative, 3=best choice, requires fast cpu
HoursFromUtc    0               Offset from utc -24 < HoursFromUtc < 24
LocalEcho       Yes             Turn off if you see double characters (lliikkee tthhiiss)
Latitude        41.15           Your latitude for accurate bearings info
Longitude       71.24           Your longitude for accurate bearings info
MaxQsos         1500            500 < MaxQsos < 9999
Name            -none-          Your name
Power           0               Output power
PrintEachContact Yes            Print each qso to your LPT
PutMsgs         Yes             Yes to show "-dx -zn" etc on screen.
Qth             -none-          Your state, province, or other qth indication
QuoteCall       No              Yes is like the "older" versions
RecordData      No              Copy incoming rtty to data file
Registration    DEMO            Your personal registration number
Street          -none-          Your street
State           -none-          Your state/province/etc
SpaceTab        Yes             Use SPACE inlieu of to TAB <space> to TAB the fields
UsualRst        59              Without the '9' for tone please!
ZipCode         -none-          Your zip/postal code/etc

[COMx]

Item            Default         Comments
-------------   --------------  -------------------------------------------
BaseAddr                        Depends on hardware installed
BaudRate        9600            300-115,200
DataBits        8               7,8
HandShake       None            None, Rts, Dtr, Xon
IrqNumber                       Depends on hardware installed
Parity          NoParity        None, Even, Odd, Space, Mark
StopBits        1               1,2


[RADIO]

Item            Default         Comments
-------------   --------------  -------------------------------------------
ComPort         None            Depends on hardware installed
Poll            1               Check radio every POLL seconds
Type            None            Depends on hardware installed
80              3600            Favorite frequency for quick band change
40              7080               "           "          "       "
20              14080              "           "          "       "
15              21080              "           "          "       "
10              28080              "           "          "       "


[CLUSTER]

Item            Default         Comments
-------------   --------------  -------------------------------------------
AllowAnySpot    Yes             Show all spots, regardless if RTTY or not
Beep-ok         Yes             Beeps, yes or no
Beep-Frequency  1000            In hertz
Beep-Duration    250            In milliseconds
CurrentBand     Yes             Show spots for band you are on
ComPort         -none-          Depends on hardware installed
FileName        Cluster.txt     Name of disk file
Loose           Yes             Use wf1b's judgement if it might be RTTY
NumSpots        10              Number of spots to hold onto
OtherBands      Yes             Show spots for other bands
SaveToDisk      Yes             Save cluster spots to disk file
SendEnter       Yes             When you start RTTY, will send enter to cluster
TTYOffset       0               If your radio is off freq, or using afsk
TTYMsg          RTTY            For use on Alt-F3 window
InputFile       SPOTS.TXT       For use with DXTelnet type programs
CommandFile     COMMANDS.TXT    For use with DXTelnet type programs
FileSeconds     30              How often to check the input file for new data


[COLORS]

Item            Default         Comments
-------------   --------------  -------------------------------------------
CatchDupe       RedOnBlack      For higlighting dupes
CatchGood       LtGrayOnBlack   For highligting need callsigns
CtrlAttr        LtCyanOnCyan    If control chars entered
FrameAttr       RedOnBlack      The window frames
HeaderAttr      LtGreenOnBlack  The window headings
HiLiteAttr      LtGrayOnBlack   Hilighting color
Message         DkGrayOnCyan    For message window
PromptAttr      CyanOnBlack     The text aids for data entry
StringAttr      DkGrayOnCyan    Input strings
WindowAttr      GreenOnBlack    Most of the test you see
RI              YellowOnBlack   K6STI RI Color

[AUTOSAVE]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Minute          00              The minute of the hour for autosave (00-59)
Path            A:\             Location for autosave, MUST be different
                                than \RTTY  (ie; C:\rtty\save\)


[EDITOR]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Insert          Yes             Insert mode
Indent          Yes             Auto indent
MakeBackup      Yes             Backup text file created
MaxFileSize     16              In kilobytes
RightMargin     77              Word wrapping column
TabSize         8               Tab space size
WordWrap        Yes             Word wrapping


[NETWORK]

Item            Default         Comments
-------------   --------------  -------------------------------------------
AutoSync        No              Send time sync messages automatically
ComportA        -none-          First serial port in network
ComportB        -none-          2nd serial port in network (if middle station)
Minute          00              Minute to perform autosync (00-59)
StationNum      0               Station identifier (1-8) must be unique
Timeout         9               In clock tics (18=1 second)



[TNC1]

Item            Default         Comments
-------------   --------------  -------------------------------------------
BaudRate        45              45 is most common
CharDelay       3               Baudot-drv only
ComPort         -none-          Depends on hardware installed
Diddles         Yes             Control diddles on or off
FilterWidth     1               0=Narrow, 1=Medium, 2=Wide
FskPolarity     Yes             Yes=Normal, No=Reverse
Mode            Rtty            For now, just Rtty
Normal          Yes             Receive polarity, Yes=Normal or No=Reverse
TxNormal        Yes             Transmit polarity, Yes=Normal or No=Reverse
StopBits        2               Baudot-drv only
Type            NONE            The type of tnc (Kam, PK-232 etc...)
Usos            Yes             Unshift on space
SquelchEnabled  Yes             Whether to enable it or not
SquelchLevel    25              Squelch level 0-127 (depends on tnc, refer to TNC manual)
Display         1               Tuning display type (HAL only!)
                                0=No Display
                                1=Zero Center
                                2=One Bar
                                3=Two Bars
                                4=Two Touch Bars
                                5=Four Bars
DisplayScale    124             Bottom range of tuning display
MarkFreq        2125            Mark frequency (some units only!)
SpaceFreq       2295            Space Frequency (some units only!)
Path            C:\             Where the Hal support files are installed
BaseAddress     $260            Location of HAL installed board
CharDelay       5               Millisecond spacing for char sent
CommandDelay    10              Millisecond spacing for commands sent
ExtraDelay      2               For very fast cpu's that can outrun the PCI-3000
CollectNumbers  No              For determing the best display scale
ZeroTuneRev     No              To make the +/- match Your tuning knob



[RECD QTC]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Alt-A           ALL AGN? BK      Message sent when alt-a is pressed
Alt-Q           <1>QRV DE <11>   Message sent when alt-q is pressed

[SEND QTC]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Alt-A           <1> DE <11> QSL? Message sent when alt-a is pressed
Alt-Q           <1> QRV? DE <11> Message sent when alt-q is pressed



[USER-DEF]

Item            Default         Comments
-------------   --------------  -------------------------------------------
CLEAR-String    -none-
RX-String       -none-          Controller to operate the radio properly.
TX-String       -none-          Enter the strings required for your demodulator


[BEEP]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Duration        250             Expressed in milliseconds (1000=1 second)
Frequency       800             Expressed in hertz
ok              yes             yes=beeps, no=silent

[CONTEST]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Ser#ByBand      No              Keeps serial numbers by band (multi-multi)



[FKEYS]

Item            Default         Comments
-------------   --------------  -------------------------------------------
F1              varies          Function key F1 through F10 are programmable
to                              for preference. Edited by entering Ctrl F7.
F10                             Ctrl Enter to save.


SF1                             Function key shift F1 through shift F10 are
to                              programmable, same as above example.
SF10

B4                              WRKED BEFORE...


[RATE]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Delta           10              Show rate for "delta" qsos
Delta2          100             Show rate for "delta2" qsos
Type=1          1               Show time rate "delta" & time since last qso
                2               Show rate for "delta" and "delta2"


[RX-SCROLLING]

Item            Default         Comments
-------------   --------------  -------------------------------------------
Increment       5               Scrolling increment
Lines           50              Number of past RX lines stored


[MOUSE]

Item            Default         Comments
-------------   --------------  -------------------------------------------
AutoScroll      No              Mouse moves up screen with incoming text
ClickStyle      0               0= original click on the first letter
                                1= click anywhere (right word preference)
                                2= click anywhere (left word preference)
                                preference=if you click on space, which way
                                RTTY will search for text
DelimSet       $20,$2C,$2D,$2E  The characters which delimit each clickable
                                item .. eg.  001-001-001 uses the - for a delimiter
                                You may enter any valid ascii character using
                                hex notation.  The defaults will be fine for
                                for most users.
                                Some common codes: $2F='/', $20=' ', $2C=',',
                                $2E='.', $2D='-'
TimeDiff       15               How "close" a time received must be to the
                                current UTC time


[PERFORMANCE]
Item            Default         Comments
-------------   --------------  -------------------------------------------
UseFriendFile   Yes             Enables operation of <HI> buffer tags
UseBearingsFile Yes             Enables operation of automatic beam heading display
UseMasterFile   Yes             Enables operation of Detectors 2 & 3, and
                                super check partial
RealTimeRate    Yes             Enables 'real time' display of QSO rate info


N O T E !
---------

If you have a slower computer, and my opinion of a slower computer is
a 386(any speed) or less than a 486/66, then here are some options to help
improve the online performance of RTTY during a contest.

Try turning off various options above(1, 2 or any and all options) to help
improve performance.  Another important consideration, is to change
the DETECTOR option (it is in the [PROFILE] section) to DETECTOR=1.



