Circuit: * D:\Simulações no LTspice\TL431\TL431_Zo_TestBench.asc

WARNING: Node IN is floating.

Direct Newton iteration failed to find .op point.  (Use ".option noopiter" to skip.)
Starting Gmin stepping
Gmin = 10
Gmin = 1.07374
Gmin = 0.115292
Gmin = 0.0123794
Gmin = 0.00132923
Gmin = 0.000142725
vernier = 0.5
vernier = 0.25
vernier = 0.125
vernier = 0.0625
Gmin = 0.000138367
vernier = 0.03125
vernier = 0.015625
vernier = 0.0208333
Gmin = 0.000136392
vernier = 0.0277778
Gmin = 0.000128154
vernier = 0.037037
vernier = 0.0493827
Gmin = 0.000115451
vernier = 0.0658435
vernier = 0.0877914
Gmin = 9.78002e-005
vernier = 0.117055
Gmin = 7.54162e-005
vernier = 0.156073
vernier = 0.208098
Gmin = 4.89353e-005
vernier = 0.277464
vernier = 0.369952
Gmin = 2.4773e-005
vernier = 0.493269
Gmin = 8.65562e-006
vernier = 0.657691
vernier = 0.876922
Gmin = 1.57141e-006
vernier = 1
Gmin = 1.77353e-007
Gmin = 1.90431e-008
Gmin = 2.04474e-009
Gmin = 2.19552e-010
Gmin = 2.35743e-011
Gmin = 2.53127e-012
Gmin = 2.71793e-013
Gmin = 0
Gmin stepping succeeded in finding the operating point.

Ignoring empty pin current: Ix(u1:11)
Ignoring empty pin current: Ix(u1:11)

Date: Fri Dec 04 13:37:29 2015
Total elapsed time: 0.315 seconds.

tnom = 27
temp = 27
method = trap
totiter = 1475
traniter = 0
tranpoints = 0
accept = 0
rejected = 0
matrix size = 92
fillins = 69
solver = Normal
Matrix Compiler1:     596 opcodes
Matrix Compiler2: 8,94 KB object code size  2.2/4.4/[2.4]


