// -----------------------------------------------------------------
// PERSEUS RECEIVER CONTROL DLL FOR WINRAD
//
// SOFTWARE RELEASE NOTES
//
// Version: 	2.3b
//
// Date: 	18 July 2012
//
// -----------------------------------------------------------------

NEW FEATURES

- The control DLL now supports also the following sample rates:

  a. 95.238 ks/S (used by Joe Taylor's K1JT MAP-65)
  b. 48 kS/s
  c. 96 kS/s
  d. 192 kS/s

  Since the digital down converters cores of the Perseus receiver
  do not implement fractional decimation and the A/D converter sampling
  frequency is 80 MHz, these rates are only approximate.
  The MAP-65 rate is obtained dividing the ADC clock by 840.
  The 48, 96 and 192 kS/s rates are obtained dividing the ADC clock by
  1664, 832 and 416.

- The new perseususb.dll with WinUSB drivers support.
  Users which wishes to use the Perseus receiver with Winrad should either 
  install the WinUSB drivers provided with the Perseus software (v2.1h)
  on their system or continue to use the perseususb.dll provided with
  older distributions and the old CyUsb.sys driver.

BUGS FIXED

- The DLL checks for the Perseus hardware at software startup as per
  the ExtIO_xxx Winrad DLL specifications.
- The DLL GUI is shown correctly when the unhide "H" key is pressed in Winrad

NOTES

- The record button of the Perseus receiver control panel has been mantained
  for compatibility with the Perseus wav file format.
  Files recorded with the Winrad Rec button are not compatible with the
  format used by the Perseus software.

- All the files of this distribution should be copied to Winrad's folder

Files included in this distribution:

- ExtIO_perseus.dll	Perseus receiver control DLL for Winrad v2.3a
- perseususb.dll        Perseus control DLL. Version 3.2 for WinUSB drivers
- perseus2m24v21.sbs	Perseus receiver config data - 2 MS/s DDC
- perseus1m24v21.sbs	Perseus receiver config data - 1 MS/s DDC
- perseus500k24v21.sbs	Perseus receiver config data - 500 kS/s DDC
- perseus250k24v21.sbs	Perseus receiver config data - 250 kS/s DDC
- perseus125k24v21.sbs	Perseus receiver config data - 125 kS/s DDC
- perseus95k24v31.sbs	Perseus receiver config data - DDC for MAP-65
- perseus48k24v31.sbs	Perseus receiver config data - 48 kS/s DDC
- perseus96k24v31.sbs	Perseus receiver config data - 96 kS/s DDC
- perseus192k24v31.sbs	Perseus receiver config data - 192 kS/s DDC


Have fun,
Nico Palermo - IV3NWV
_______________________________________________________________________________

(c) 2007,2009 Microtelecom s.r.l. - Pavia di Udine, Italy - All rights reserved
