KPG-7D help message file [KPG7D.HLP]
VERSION 2.00
RELEASE 4/1/1996
    Add some models for new FCC PART90.
    Wide/Narrow selection per channel.

H.0 [F1- HELP]****************************************************************


	H.1 *** [ General Help ] ***
 Along the top border of the main program screen (Channel Info.) are
 the "drop down" menus (press ALT; use the cursor keys --> <-- to  select
 a program section. Help is available for each menu by pressing the F 1
 function key. Pressing F1 while in the Channel Info. screen will load
 it's Help screen. To get familiar with the computer key functions used
 in the KPG-7D, hit ALT now; select Keyboard Help; hit ENTER. Within
 a Help  screen use cursor up/down to scroll; F5 to print a hardcopy; and
 ESC or ALT to escape the screen. Refer to the KPG-7D Instruction Manual
 for additional help. 

**Basic Use Instructions (use F1 for Help in each program section below)*

A. [CREATING PROGRAMMING DATA FOR A MOBILE]
  1. Open "MODEL" menu and select the appropriate model type.
  2. Open "EDIT-Key Selection" menu and assign a function to keys on the
     control head. (hint: use ALT to return to EDIT menu)
  3. Open "EDIT-Scan Information" menu; set SCAN features & parameters. 
  4. Open "EDIT-Feature Option" menu; set the general built-in features.
  5. Hit ESC; the cursor will move the main screen, "CHANNEL INFORMATION"
     set all per-channel and/or channel group information.
B. [PROGRAM A RADIO]
  1.  Open the "PROGRAM" menu.
  2.  Select "Write to radio".
C. [SAVE PROGRAMMING DATA TO DISK FILE]
  1. Open "FILE" menu.
  2. Select "SAVE" for quick save to the "default" or "current" filename.
     or "SAVE AS" to name or rename the file.. 

   *Organizational Chart of the KPG-7D*****
 
 [ MAIN SCREEN ]
 (   )- MENU BAR
 (0.0)- CHANNEL----+-- Channel Name (Alphanumeric Display Inf.)
      INFORMATION  +-- Receive & Transmit Frequencies 
 |                 +-- Wide/Narrow 
 |                 +-- QT/DQT Decode & Encode 
 |                 +-- Channel Delete/Add for Scan
 |                 +-- Group Delete/Add for Group Scan
 |                 +-- Option Signaling (2-tone or DTMF decode boards)
 |                 +-- Scrambler Y/N (Y=enabled, N=disabled)
 |                 +-- Scrambler Code (CODE 1-16;4bit BCD)
 |                 +-- Priority Ch. and Home Channel set
 |                 |     (press F10 to set Home Ch and Fixed P1 & P2)
 |                 +-- (IF Frequency & Ch Step) (CAUTION: DO NOT USE)
 | 
 (1.0)- FILE ----+-- New
 |               +-- Load
 |               +-- Save As
 |               +-- Delete
 |               +-- Print
 |               +-- Exit
 |
 (2.0)- MODEL----+-- Basic 32 Ch
 |               +-- Basic 32 Ch w/Alphanumerics
 |               +-- Basic 99 Ch
 |               +-- Basic 99 Ch w/Alphanumerics
 |               +-- Full  32 Ch (Alphanumerics standard)
 |               +-- Full 160 Ch (Alphanumerics standard)
 |
 (3.0)- EDIT-----+-- Key selection---+- Basic control Head
 |               |                   +- Full featured Control Head
 |               |
 |               |
 |               |
 |               |
 |               +-- Scan -----------+- Resume Time A
 |               |   Information     +- Off Hook Scan
 |               |                   +- Resume Time B
 |               |                   +- Priority 1
 |               |                   +- Priority 2
 |               |                   +- Look Back Time A
 |               |                   +- Look Back Time B
 |               |                   +- Revert Channel
 |               |
 |               +-- Feature Option--+- Time Out Timer
 |               |                   +- Busy Channel Lock Out
 |               |                   +- Off Hook Decode Enable
 |               |                   +- Power On Tone
 |               |                   +- Control Tone
 |               |                   +- Warning Tone
 |               |                   +- Roll Over
 |               |                   +- Priority Ch Temporary Delete
 |               |                   +- Scramble Code Selectable
 |               |                   +- Tx Audio Monitor
 |               |                   +- Operator Selectable Tone(QT/DQT)
 |               |
 |               +-- Embedded Message
 |                              (40 characters max. electronic serial #)
 |
 (4.0)- PROGRAM -+-- Read From Radio
 |               +-- Write To Radio
 |
 (5.0)- SETUP----+-- Communication Port
 |               +-- Display Color
 |               +-- Help Path
 |
 (H.O)- HELP-----+-- (H.1)GENERAL HELP
                 +-- (H.2)COMPUTER KEYBOARD HELP


	H.2 *** [ Computer Keyboard Help ] ***
 Currently available keys functions are displayed on the bottom screen
 border.

 ESC: returns to the main screen; Channel Information
      (exits menus & sub-screens).
 ALT: "Go to Menu" or "Go back" to previous screen.
 CURSOR Keys: moves cursor within a data input field;
              scrolls help screens.
 PgUp & PgDn:  pages up/down Channel Group & Help screens.
 F1: Opens a Help screen.
 F2: through F10: Selects labeled functions in shown at screen bottom.
      F2: Toggles Yes/No or increments selection in data fields.
      Shift+F2: Decrements selection in data fields.
      F3: Copies the current channel data to another channel.
      F4: Copies a RX frequency column entry to the TX frequency column.
      F5: Prints the current Help screen.
      F7: Next page/ channel group (same as page up)
      F8: Previous page/ channel group (same as page down)
      F10: Home channel and Priority channel set
      Shift+F3: Copies an entire channel group to other channel group.
      Shift+F4: Copies a QT/DQT decode column entry to the encode column.
      Shift+F9: Channel Insert (inserts a blank channel row & advances
                the current channel data & all subsequent channels to
                the next channel row).
      Shift+F10: Channel Delete (deletes the current channel data row
                 and decrements all subsequent channel rows by one.
 HOME: jumps to channel 1 of the Channel Info. screen, or to page 1 of
       a help screen.
 END: jumps to last channel in Channel Info. screen, or to last page of
      a help screen.
 ENTER: enters data into a program field, or opens a selection window.
 SPACE BAR: toggles Yes/No selections, or increments selections.
            (same as F2)

	0.0  [ CHANNEL INFORMATION HELP ]

 0.1- Channel Name (Alphanumeric Display Information) 
  Enter the channels receive frequency first. Available on:   
  KCH-3 BASIC front panels (w/KCH-5 EEPROM option); 2 characters max.
  KCH-4 FULL featured front panels (factory) 12 characters max.

 0.2- Frequency
  Type Receive and Transmit frequencies directly. Receive-only channels
  are allowed. Frequencies must be within the displayed band range and
  of the proper PLL channel step.
  0.2.1- W/N
   Wide/Narrow selection for W/N model only.
    Type "W" or "N".
    -Or- 
    Hit ENTER to open window and select W/N with cursor.
    -Or- 
    Hit F2 key or SPACE BAR to change alternately.

 0.3- QT/DQT Decode-Encode
  QT: 67.0 Hz to 250.3 Hz  (in 0.1 Hz steps)
  DQT: codes 023 to 754 (defaults to Normal codes)
  enter D###N  (Normal)   D###I (Inverted)
    Type tone or code directly. 
    -or-
    Hit F2 key, open QT/DQT chart, then select.

 0.4- SCN D/A
  Add: Adds the channel to SCAN map. (default)
  Del: Deletes the channel from SCAN map.
    Type "D" or "A". 
    -Or- 
    Hit ENTER to open window and select D/A with cursor.
    -Or- 
    Hit F2 key or SPACE BAR to change alternately.

 0.5- OPT SIG
  (Install an OPTional SIGnalling unit & KCK-5 interface board) 
  KDS-8B (tunable) or KDS-10 (P.C. programmable): 2-tone decoders
  KDD-4: DTMF decoder
  Enable (Y) or disable (N) this decoder board per channel. If QT or DQT
  decode is also programmed, both OPT SIG(Yes) & QT/DQT tones must be
  decoded for audio to unmute. 
    Type "Y" or "N". 
    -Or- 
    Hit ENTER to open window and select Y/N by cursor.
    -Or- 
    Hit F2 key or SPACE BAR to change alternately.

 0.6- [SCRAMBLER] (Enables/disables, per ch., a scrambler or signaling
  board at CN108)
  0.6.1- V/SC: enables/disables the scrambler per channel.
    Type "Y" for enable or "N" for disable
    -Or-
    Hit F2 key or SPACE BAR to change Alternately.

  0.6.2- CODE: Selects code 1 to 16(8). (BCD address code to board)
    Note: If the "Scramble Code Selectable"=Y in the Edit-Feature Option
    section of this program, then this column will not be available.
    Type a number from 1 to 16(8).
    -Or-
    Hit F2 key to increment selections.

 0.7- [ Shift+F6-IF FREQUENCY AND FREQUENCY STEP ] <CAUTION! CAUTION!>
  Shift+F6 key opens the selection window.
  0.7.1-  IF Frequency: fixed by hardware; DO NOT CHANGE!!!- FOR FACTORY
          USE ONLY. Must be set as follows:

        VHF LOW  = 10.7   MHz
        VHF HIGH = 34.4   MHz
        UHF      = 69.375 MHz 
   
  0.7.2- Frequency Step: selectable; can select either PLL channel step

        VHF LOW  =  5.0 kHz or  6.25 kHz
        VHF HIGH =  5.0 kHz or  6.25 kHz
        UHF      = 12.5 kHz or 10.0  kHz(requires modification)

 0.8- [F10-Home Ch and Priority Ch set]
  Select a channel you want to set as Home channel, Priority 1 channel
  or Priority 2 channel.  
  Press F10 key to open the selection window
  Select Home channel, Priority 1 channel or Priority 2 channel by cursor
  key. Press enter to confirm.
  *** Note ***
  Home channel selection is available when HC key is selected on Front
  panel. 
  Priority channel selection is available when priority channel is
  "Fixed" or "Operator Selectable"


	1.0 *** [ FILE HELP ] ***

1.1-  NEW (CLEAR FILE)
   The NEW function clears any currently loaded, read or created data
   file. All program data screens will be set to defaults.

1.2- LOAD (OPEN FILE)  -See Note** below
   The LOAD function is used to retrieve a stored data file from a hard
   disk or floppy disk to be modified, viewed, written (program a mobile)
   or printed out. An alphabetically directory of stored files will be
   displayed to select from.

1.3- SAVE (a file)  -See Note** below
   Saves the current program data with current file name. 

1.4- SAVE AS (save with name or rename) -See Note** below
   Saves with the option of assigning a "new" file name, or rename an
   existing file.

1.5- DELETE FILE  -See Note** below
   The DELETE function is used to remove any stored data files from the
   directory of stored files.

 Note**: The program will prompt for the correct drive and path statement
 where stored files are to be retrieved from; the default- A:\KPG7D\DATA 
 will be used if not re-written; this statement can be changed at any
 time and will be saved until re-written. 

1.6- PRINT FILE
   Prints all radio programming data currently loaded into the program:
    - Model Type 
    - File Name
    - Embedded Message
    - Model Type Configuration
    - Key Selection
    - Scan Information
    - Feature Option
    - Frequency Step
    - Priority Channel Information
    - Channel Information

1.7-  DOS (Prompt)
   Go back to the DOS prompt temporally. Type EXIT and press ENTER to
   quit the DOS prompt and return to KPG-7D.

1.8-  EXIT TO DOS
   Quits this program and returns to the DOS PROMPT.



	2.0 *** [ MODEL HELP] ***
 (Selects the proper mobile model & configuration)

2.1- [FRONT PANEL TYPE & CHANNEL/ALPHANUMERIC CAPABILITY ]
   Basic 32ch    - (KCH-3) Basic front panel(s), 32 Channels   [factory]
   Basic 99ch    - (KCH-3) Basic front panel(s), 99 Channels
                                                          [mod. w/KCH-5]
   Basic 32ch AN - (KCH-3) Basic front panel(s), 32 Channels
                   w/ 2 character Alphanumeric Display    [mod. w/KCH-5]
   Basic 99ch AN - (KCH-3) Basic front panel(s), 99 Channels
                   w/ 2 character Alphanumeric Display    [mod. w/KCH-5]
   Full  32ch    - (KCH-4) Full Featured front panel(s),       [factory]
                   32Ch. (2grps x 16ch.s)
                   w/ 12 characters Alphanumeric Display
   Full 160ch    - (KCH-4) Full Featured front panel(s),
                   160Ch. (10grps x16ch.s)
                   w/ 12 characters Alphanumeric Display  [mod. w/KCH-5]

 2.1.1- CONTROL HEAD (number of control heads)
    Single Control Head- for under-dash or 1 head configurations.
    Dual Control Head- for KRK-3DH dual head kit installed.

 2.1.2- BAND (number of RF Bands (RF decks) in the mobile configuration;
    VHF high, VHF low or UHF)
     Single Band - 1 RF Band
     Dual Band   - 2 RF Bands (requires KRK-4DB kit installed)

 2.1.3- RADIO BAND (enter the frequency range of each RF deck used)
    Changing the band(s) after selected will erase all previous channel
    data. 
  Note: Dual Band configured mobiles cannot have 2 of the same band.

   VHF low band   K   29.7- 37  MHz
                  K2  35  - 43  MHz
                  K3  41  - 50  MHz
                  Special Tune (29.7 - 50 MHz; factory use only)

   VHF high band  K   150 - 174 MHz
                  K2  136 - 156 MHz
                  Special Tune (136 - 174 MHz; factory use only)
                  Wide/Narrow model available for each band.

   UHF band       K   450 - 470 MHz
                  K2  470 - 490 MHz
                  K3  490 - 512 MHz
                  K4  403 - 430 MHz
                  Special Tune (400 - 520 MHz; factory use only)
                  Wide/Narrow model available for each band.

 2.1.4- VOICE SCRAMBLER UNIT INSTALLED? (or signaling board at CN108)
    Applicable per RF deck. If "Y" (yes) is selected, the "Scrambler-
    V/SC-Code" column appears in the Channel Info. screen. The board can
    be enabled/disabled and set for 1 of 16(8) codes on a per ch. basis.
    See service manual for details.

	3.0 *** [ EDIT HELP ] ***

 Index of Edit Help Messages (use PgUp/PgDn for quick access)
 + KEY SELECTION ------------------section 3.1
 + SCAN INFORMATION ---------------section 3.2
 + FEATURE OPTION------------------section 3.3
 + EMBEDDED MESSAGE----------------section 3.4
 
3.1- [KEY SELECTION]  (Front panel keys)
  This screen displays the type of front panel that was selected in the
  "MODEL" type configuration section. Each "boxed" control key shown is
  programmable for 1 of 13 possible functions, or "No" function.
  (The Monitor and Scan keys default to the "Monitor" & "Scan" functions
  respectively, since they are generally used this way.
  (KCH-4: KEYS 3 to 4 default to "No" function if left unprogrammed.)
  Two type of Front panel are available.
  KCH-3 BASIC Front: 4 Programmable Keys (2 characters LCD; internal
        speaker)
  KCH-4 FULL-FEATURED Front: 6 Programmable Keys (12 characters Alpha-
       numeric LCD; group up/down switch)
 <!>Note: For Dual Head configurations, both fronts must be of the same
          type.

  Use the following computer keys to program:
  1. Open "KEY SELECTION" section; the front panel is displayed .
     UP/DOWN & LEFT/RIGHT ARROW: selects the panel keys to be programmed.
  2. a) Hit ENTER to open KEY SELECTION "function list"
        UP/DOWN ARROW: selects the function
        Hit ENTER to confirm it.
        Hit F10 for the  OPT & AUX keys function assignment-see below**.
       -or- 
     b) F2 or Space bar: to increment the selections inside the
        individual keys Hit F10 for the OPT & AUX keys function
        assignment-see below**.

 ** Key Function list

 BLANK: No function
 MON: MONITOR ON/OFF; enables /disables QT/DQT tone squelching
 SCN: SCAN MODE ON/OFF; turn on and off SCAN mode.
 HC: HOME CHANNEL; Jump to the Home channel.
 PA: PUBLIC ADDRESS ON/OFF; RF deck accessory jack pins 12 & 6 function
     as a 13W PA (20W max.) <!>-Requires 20W rated speaker (KES-4). 
 HA: HORN ALERT ON/OFF; for 2-Tone & DTMF options only.
 TA: TALK AROUND ON/OFF; simplex operation (receive frequency) on any
     programmed channel.
 IC: INTERCOM ON/OFF; for IC on Dual Control Head configurations only.  
 AN: ALPHANUMERIC DISPLAY ON/OFF; Toggles between the programmed CHANNEL
     NAME(Alphanumeric characters) and Grp/Ch number in the LCD.
 SP: SPEAKER CONTROL: Switches RX audio from the Panel/Control Head 
     speaker(s) to the PA output speaker. (See service manual)
 D/A: DELETE/ADD; For "User-selectable" D/A of channels/groups in
      the scan map. See instruction manual for details
 SQL: Allows mobile operator to select noise squelch level.
 OPT: Programmable for 1 of 3 functions below**
      (default: V/Scramble) / Press F10 
 AUX: Programmable for 1 of 3 functions below**
      (default: Aux. Output) / Press F10
      **Select one of these three following functions.
     1. Operator-selectable Voice Scrambler Control:
        Allows mobile operator to select any 1 of 16(8) pre-programmed
        codes in the scrambler unit and manually activate it when needed.
        The code selection is memorized until changed.
        (for V/Sc or a BCD addressable signaling board installed at
        CN108- see service manual for details and operation)
        
     2. Operator-selectable Tone(QT/DQT) Control:
        Allows mobile operator to select 1 of 16 tone/code pairs from
        the pre- programmed tone/code list in the Edit-Feature Option
        section this program and manually activate it when needed.
        The selection is memorized until changed. 

     3. Auxiliary Output Control:
        (see service manual for details: Auxiliary Function)
        Provides on/off control of Q116 (open-collector, sinks 100mA)
        used for peripheral device control (ex: relays, lights, etc.).
        Factory set for LCD back-light on/off. Can be PCB set for open-
        collector output at control head rear accessory plug.


3.2- [ SCAN INFORMATION ]

 3.2.1- RESUME TIME A & B:
  Scan resume time interval from the end of a received call to the time
  scan automatically resumes. (0 to 5 sec. @ 0.1 second steps)
  [Resume time A] is active while on hook normal scan 
  [Resume time B] is active only while off hook scan is selected.

 3.2.2- OFF HOOK SCAN:
  If enabled-"Y", the mobile is able to scan even though the mic
  is off hook.  default: "N" 

 3.2.3- PRIORITY 1 & 2: (program choices for both P1 and/or P2)
  a) None-No priority ch.; If P1=None ,then P2=None automatically
  b) Fixed-A fixed channel (set by this computer programming ONLY).
  c) Selected CH.- The currently selected channel via the channel or
                   group/channel controls.
  d) Operator Selectable- Operator can "program" the pri. ch. from the
     front panel keys.
     To set P1: select ch., hold Scan key, hit Monitor key 3 times.
     To set P2: select ch., hold Scan key, hit Monitor key 2 times. 
     To set P1 or P2 to "None": use above procedure, except hit D/A key.
    Note: Only one P1 and one P2 can be programmed, even for multi-group
    mobiles

 3.2.4- GROUP SCAN:
  (KCH-4 Full featured panels only; 2 g. x 16 ch., 10 g. x 16ch.)
  [Single]- Scans only the currently selected channel group.
  [Multi]- Scans all channel groups (added groups & ch.s).

 3.2.5- LOOKBACK TIMES:
  Priority channel checking intervals while receiving on a non-priority
  channel. The mobiles CPU chooses either Lookback time A or B depending
  on the priority channel activity--Program both times.
  [Lookback A]: Priority channel is not busy (no carrier present).
  This time is typically set shorter than Lookback B, since the priority
  ch. should be checked more often so as not to miss a call.
  Lookback A: 350-2900ms in 50ms steps; default=350ms
  [Lookback B]: Priority channel is busy, but tone squelched.
  This time is typically set long since the priority ch. is busy with 
  a user with a different tone.
  Lookback B: 350-5450ms in 50ms steps; default=2050ms

 3.2.6- REVERT CHANNEL (for this program list-hit ENTER to open window):
  Revert Ch. is the programmable off-hook destination channel. The
  choices made available in the screen are dependent on two factors:
  (1) Whether P1 and/or P2 are used (P1 only, both or neither)
  (2) How P1/P2 are set (fixed, selected, Operator-selectable.)
  The choices made available will be 3 or more of the following:
  (a) Selected Ch.- Channel selected by controls prior to scan
      initiation.
  (b) Last Called Ch- last channel a call was received on.
  (c) Last Used Ch.- last channel a transmission was made on.
  (d) P1
  (e) P2
 *(f) P1 > P2
 *(g) P1 > P2 > Last Called Ch..
 *(h) P1 > P2 > Last Used Ch.
 *(i) P1 > P2 > Last Selected Ch.

  *[f to i]: Are sequences made available when one or both priorities
  are set for "Operator Selectable". In these sequences, if a priority
  channel is "de-selected as a priority ch; i.e., set to None", then
  the next listed channel becomes the Revert Channel.
  *[g,h,& i]: if either priority is set for "Fixed", then it will not
  appear in these sequences on the program screen.


3.3- [ FEATURE OPTION ]

 3.3.1- TIME OUT TIMER: TX time out is able to set from 15 to 225 seconds
  in 15 sec. steps. default: OFF

 3.3.2- BUSY CHANNEL LOCKOUT: TX inhibited when the channel is busy.
  default: NO

 3.3.3- OFF HOOK DECODE ENABLE:
  If enabled-"Y", the mobile is still tone squelched even though the mic
  is off hook (valid for QT/DQT decode, 2-Tone & DTMF decode options).
  default: "N" (off hook condition disables decoder)
  Note:
  (a) This only "disables" the effect the mic-hook condition has on
      the "monitor" condition. For the 2-Tone & DTMF options, hitting
      PTT or the monitor key will disable their muting. 
  (b) The mic-hook condition still starts & stops scanning. The Off-hook
      Revert Channel function is still valid (see Scan Information).

 [Supervisory Tones]: User friendly acknowledge and warning beeps.
 "Yes" is enabled and "No" is disabled.]                               
 3.3.4- POWER ON TONE: Beep tone at radio power up. 

 3.3.5- CONTROL TONE : Key and selector knob echo-back beeps.

 3.3.6- WARNING TONES: PLL unlock, Time-out timer & Busy ch lockout
  alert tones

 3.3.7- ROLL OVER: channel knob selection method. 
  Yes- Channel Rollover: continuous channel selection with no stops.
  No-  First & last channel electronic stop: selection attempts past the
       first or last channel are prevented and also indicated with an
       audible speaker beep.

 3.3.8- PRIORITY CHANNEL TEMPORARY DELETE ENABLE:
  Normally, the priority channel cannot be deleted from the scan map via
  the "temporary delete" feature. If "Yes" is chosen, this is overridden.
  Hold D/A key for two seconds to delete the priority channel temporary
  when scan stops on it. The Priority Ch. will remain deleted until the 
 "Scan" mode is cycled off/on.

 3.3.9- TX AUDIO MONITOR: (Dual control head configuration only)
  Enables monitoring of the transmission audio from the active control
  head by the idle control head.
  Yes- enabled, No- Disabled

 3.3.10- SCRAMBLE CODE SELECTABLE:
  Yes- enables the Operator-selectable 1 of 16(8) code feature, BUT
  disables the pre-programmed  per channel code settings in the Channel
  Info. screen- Scrambler Code column (this column will disappear).
  See service manual for details. 
  No- disables this feature; the per channel programming can be used.

 3.3.11- OPERATOR SELECTABLE TONE(QT/DQT) (16 code menu) 
  This feature is made available ONLY after a front panel key has been
  assigned for this feature in the Edit- Key Selection section (3.1)
  Allows the operator to select 1 of 16 tone pairs from a "lookup" menu,
  then activate it manually (regardless of the pre-programmed tone pair
  in the Channel Info. screen). See service manual for details.
  Hit enter; a blank 16 code menu for operator-selectable tone pairs
  is displayed for fill-in. 
  Type:
     QT: 67-250.3 @ 0.1 Hz 
     DQT: 000-777 Normal or Inverted. 
     -or-
     Hit F2; cursor-select from the EIA standard lists


3.4- [ EMBEDDED MESSAGE ]
  Up to 40 alphanumeric characters can be programmed into each mobile.
  This can be used for an electronic serial number, program file name
  notation, property ID., etc.. It will appear as part of the header
  statement on a program data printout along with the model type and
  filename.

	4.0 *** [ PROGRAM HELP ] ***

For Reading and writing between computer & mobile:
a) SET THE RADIO IN PROGRAM MODE:
   -Radio power off.
   -Hold down the OPT (KCH-3 BASIC front) or KEY1 (KCH-4 FULL front)
    button while powering up the mobile (power switch).
   -Keep the OPT/KEY1 held down more than 2 seconds
   -When  "PG" (KCH-3 BASIC front) or "PROGRAM" (KCH-4 FULL featured
    front) appear in the LCD, release the OPT/KEY1 button.
   -Mobile is now in program mode (it will not RX, TX or function
    normally).

b) CONNECT THE KPG-4 INTERFACE CABLE:
   DB-25 connector to the computer's serial port (COM1 or COM2) and
   the RJ-11 modular end to mobiles mic jack. 

c) READY FOR READ/WRITE OPERATIONS (Note: Be sure that the COM level in 
   the Setup (5.1) section of this program is properly set to match that
   of your computer.)

4.1- READ PROGRAM DATA FROM RADIO
 Reads all program data from the radio--select & hit enter.
   
4.2- WRITE PROGRAM DATA TO RADIO
 Writes all currently loaded program data into the mobiles EEPROM memory.
 Verify that the model type & configuration in the current data matches
 that of the target mobile you are about to program.



	5.0 *** [ SETUP HELP ] ***
5.1- COMMUNICATION PORT
 Select the COM level of the computer's serial communication port for
 programming. There are two choices, COM1 or COM2. COM level setting's
 in your computer may be dependent on internal hardware and/or setup
 software settings; check you computer manuals for details.

5.2- DISPLAY COLOR
 Select Color or Black & White.
  Color- color schemes for each screen display element(below) can be set.
  You can choose one of eight colors to an element. 

   Display element:
    Display background color
    Input data color
    Feature highlight color
    Screen border information color
    Windows menu bar color
    General message color
    Windows color 
  Black & White (default)- best suited for monochrome & B/W displays.

5.3- HELP PATH (FILE DRIVE AND SUB-DIRECTORY PATH)
 Help message files are contained in this program under KPG7D\KPG7D.HLP 
 The drive and path statement that this program uses to access these 
 messages is initially set to A:\KPG7D. 

 

