F1 - MAIN HELP SCREEN                                                           E>  Conventions:                                                              <E                                                                                    <key> indicates a single "key" is required to be pressed, e.g. <X> means        press  the  X  key  only.                                                                                                                                       ^key indicates that the "key" must be pressed after pressing and holding        the control (<Ctrl>) key e.g. ^L means press the <Ctrl>  THEN  L  keys.                                                                                                                                                                     E>  Commands:                                                                 <E                                                                                    The  KFT-x  programmer  has  the  following  commands  available:                                                                                               COMMAND KEY               FUNCTION                                              ------------------------------------------------------------------------        <F1>      Help Screen     Description of features (this file)                   <F2>          ^           Toneset table reference screen                        <F3>          |           KFT-x Interface Details                               <F4>          |           Tone Formats                                          <F5>          |           Special Tone Formats                                  <F6>          |           Operating Instructions                                <F7>          |           Electrical Specifications                             <F8>          |           Error conditions                                      <F9>          v           List full customer setup directory                    <F10>     Help Screen     Display Handbook                                                                                                                      ^H                        Help window for highlighted parameter                                                                                                 <Up>/<Down>               Backup 1 line / Advance 1 line                        <PgUp>/<PgDn>             Backup 10 lines / Advance 10 lines                    <Home>/<End>              Go to START of table / Go to END of table             <Left>/<Right>            Select option                                                                                                                         <+>/<->                   Increment / Decrement fully-numeric parameter                                                                                         <W>                       Write current setup to S1516                          <R>                       Read setup from KFT-x into current setup              <V>                       Verify setup in KFT-x with current setup                                                                                              ^O                        OOPS Return previous setup after Read                 ^P                        Output current setup to printer                       ^S                        Save current setup to disk SETUP file                 ^L                        Load current setup from disk SETUP file               ^D                        Delete disk SETUP file                                                                                                                ^E or ^Q                  Exit program                                                                                                                          ^C                        Software Configuration                                                          - Specify Drive (and directory) for SETUP files                                 - Set display to Colour or B&W (Monochrome)                                                                                       