G4ALN Penny Feed measured at 10.368 GHz

Dish diameter = 10 λ Feed diameter = 0.98 λ

E-plane

H-plane

0 dB -10 -20 -30

N1BWT 1997

0.3 0.4 0.5 0.6 0.7 0.8 0.9

0.25 1.0

10

20

30

40

50

60

70

80

90

1 dB

2 dB

3 dB

4 dB

5 dB 6 dB 7 dB 8 dB

MAX Possible Efficiency AFTER LOSSES: REAL WORLD at least 15% lower Illumination Spillover Feed Blockage

Parabolic Dish f/D

Efficiency %