openspot
Loading...
Connecting to openSPOT...

# Login

Password:
Remember me

# Status

To: 226123
From: YO2LIC (2262002)
Group DMR voice call from net
At: 21:15:26 (length: 00:10)
(talker alias)
To:
From:
At:
No call log entries
Status:
standby
Active config profile:
0 (DP4801E-BM DMR)
Changing to profile in:
Active connector:
Homebrew/MMDVM
Changing to null connector in:
Modem mode:
DMR/Hotspot
Modem RX/TX frequency, power:
438.025000/438.025000 100%
Connected to:
9990
Server:
primary
Homebrew call rerouting:
not active
BrandMeister linked static TGs:
226, 2260, 2262, 2263, 2264, 2265, 2266, 2267, 2268, 2269, 9800, 22601, 22603, 98010, 226112, 226123
BrandMeister linked dynamic TGs:
-
BrandMeister linked reflector:
-
BrandMeister server:
status list active groups last heard

# openSPOT info

Hardware version:
v1.1 (433 EU)
Software version:
0141
Bootloader version:
0004
MAC address:
FE:28:FB:79:16:CF
Device ID:
FB7916CF
Uptime:
1 day, 08:31:54

# SharkRF IP Connector Server

Connected client ID:
Connected client callsign:
RSSI ▸
BER ▸
Network UDP traffic ▸
Dejitter queue ▸

# Connectors

Active connector:
Homebrew/MMDVM
Edit connector:

## General settings

Change to null after last RX call (sec, 0 to disable):

## Quick call

Destination ID:
Group call Private call
TDMA channel:
0 1

## BrandMeister manager

### API key

API key:

### Actions

### Static talkgroups

Add static talkgroup ID:
Currently linked static TGs:
226 ❌, 2260 ❌, 2262 ❌, 2263 ❌, 2264 ❌, 2265 ❌, 2266 ❌, 2267 ❌, 2268 ❌, 2269 ❌, 9800 ❌, 22601 ❌, 22603 ❌, 98010 ❌, 226112 ❌, 226123 ❌

### Dynamic talkgroups (use quick call to link/unlink)

Currently linked dynamic TGs:
-

### Reflector

Active ID (4000 - not linked):

## Null connector

Modem receive frequency (MHz):
Modem transmit frequency (MHz):

## DMR/DMRplus dongle

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Server:
Server address:
Port:
DMR ID:
Reflector:
Reflector ID:
Keepalive interval (sec):
RX timeout (sec):

## DMR/Homebrew/MMDVM

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Protocol:
Homebrew MMDVM
Server:
Server address:
Port:
Callsign:
DMR ID:
URL:
Server password:

Backup server:
Backup server address:
Backup server port:
Backup server password:
Backup server activate connect timeout (sec):

Auto connect to ID (0 to disable):
Group call Private call
Disconnect TG/ref. on auto connect
Auto connect TDMA channel:
Auto connect interval (sec):

DMO mode TDMA channel:
Route C4FM calls to ID:
Group call Private call
Reroute DMR TG9 calls to ID (0 to disable):
Group call Private call
Keepalive interval (sec):
RX timeout (sec):

### MMDVM options for DMRplus

Use DMRplus options
Start reflector:
Start reflector ID:
Relink time (min):
User link allowed
Static TG #1:
Static TG #2:
Static TG #3:
Static TG #4:
Static TG #5:
Raw options:

## DMR/TS repeat

This connector has no available settings.

## D-STAR/DCS/XLX

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Server:
Module:
Server address:
Port:
CCS port:
Callsign:
Local module:
Reflector ID:
Remote module:
RX timeout (sec):

## D-STAR/REF/XRF (DPlus/DExtra)

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
List:
Reflectors Gateways
Server:
Module:
Server address:
Port:
CCS port:
Callsign:
Local module:
Reflector/gateway ID:
Remote module:
RX timeout (sec):

## System Fusion/FCS

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Server / room number:
Server address:
Port:
Callsign:
CCS7 ID:
Reflector:
Room number:
Keepalive interval (sec):
RX timeout (sec):

## System Fusion/YSFReflector

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Server:
Server address:
Port:
Callsign:
Keepalive interval (sec):
RX timeout (sec):

## SharkRF IP Connector Client

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Server:
Server address:
Port:
ID:
Password:
Callsign:
Keepalive interval (sec):
RX timeout (sec):

## SharkRF IP Connector Server

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Port:
Password:
RX timeout (sec):

## DMR AutoCal

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Status:
idle
Progress:
Last result:
N/A

## C4FM Half Deviation AutoCal

Modem receive frequency (MHz):
Modem transmit frequency (MHz):
Status:
idle
Progress:
Last result:
N/A

# DMR SMS chat

No messages
Message:
Destination ID:
Send to:
Network Modem
Call type:
Private Group
TDMA channel:
0 1
Format:
ETSI UDP UDP/Chinese Try all

# Settings

Source ID:
Intercept network messages

# Modem settings

Mode/submode:

## Frequency

Modem receive frequency (MHz):
DMR demodulation mode:
C4FM demodulation mode:
Modem transmit frequency (MHz):
Transmit power:
13 dBm (19.95 mW)

## CW ID

ID to transmit:
Speed (WPM):
Interval (sec):
TX delay (sec):

## Modulation

Modulation mode:
Bits per second:
Inner deviation (Hz):

## Packet settings

Packet size (bits):
Sync word length (bits):
Sync word pos. in packet (bits):
Sync word count:
Sync word #1 (hex):
Sync word #2 (hex):
Sync word #3 (hex):
Sync word #4 (hex):

## TDMA

TDMA enabled
TDMA calibration duration (packets):
TDMA calibration comp. multiplier:
Sync frames num. for chan. validation:

## Calibration

Auto calibration
Quick cal. delay (sec):
Autocal modem CPU temp. diff. (°C):
Autocal RF modem temp. diff. (°C):
Autocal temp. read interval (sec):
Autocal temp. read delay (sec):

## Other settings

Call hang time (ms):
RSSI average sample count:
BCLO level (dBm, 0 - off):
Sensitivity level:
Filter gain:
Auto AGC
AGC low threshold (dBm):
AGC high threshold (dBm):
External VCO

## Config profile

### Change active profile

Active profile slot:
0 (DP4801E-BM DMR)
Change to profile slot:

### Change profile on modem RX timeout

Change after last RX call (sec, 0 to disable):
Change to profile slot:

### Change name

Active profile name:

### Copy

Copy active profile to slot:

### Active profile config file

Status:
Idle
Progress:

## Web interface password

New password:

## Network settings

Hostname:
Dejitter queue length (ms):
IP configuration mode:
Static IP:
Netmask:
Gateway:
Override DHCP/auto DNS servers
DNS1:
DNS2:

## Voice announcements

Enabled
Shortened BrandMeister announcement
Use server only
Server:
Server host:
Server port:
Source DMR ID:
Profile query/change base DMR ID:
Connector query DMR ID:
IP address query DMR ID:

## Location settings

Country of operation:
QTH locator:
Latitude:
Longitude:
Height (AGL, meters):
Description (city, country):

## DMR settings

Auto update DMR ID database
Color code:
Echo ID:
Default DMR ID for C4FM calls:
Allow only DMR IDs as C4FM callsigns
Send no in-band data to network
Force talker alias to DMR network:
Send no in-band data to modem
Transmit idle in BS mode idle TX slot

## D-STAR settings

Echo callsign:
Transmit RX confirmation

## C4FM settings

Auto mute DTMF commands
Special command/cross mode private call DTMF code:
Cross mode group call DTMF code:
Transmit RX confirmation
Default callsign for DMR calls:
Only receive SQL code from modem
SQL code from modem:
Replace SQL code to modem enabled
Replace SQL code to modem:
Replace SQL code to net enabled
Replace SQL code to net:

## Lock settings

CCS7/DMR ID #1 (0 to disable):
CCS7/DMR ID #2 (0 to disable):
CCS7/DMR ID #3 (0 to disable):
Callsign #1 (empty to disable):
Callsign #2 (empty to disable):
Callsign #3 (empty to disable):