# TinTrak 4 configuration file
# You can use the following variables in this configuration file that will be 
# replaced by the actual values as configured in PinPoint during TNC init.
#
# [ESCAPE] send the ESC key. TinyTRak needs 3 ESC keys to enter config mode
# [ALIAS1] [ALIAS2] [ ALIAS3] will be set to fill-in digi path if digi enabled. TEMP if disabled
# [PATH1] [PATH2] [PATH3] is the individual path into WIDE1-1 and then WIDE2-1 for example
# [MYCALL] sets the user's callsign including SSID, e.g. AB0WV-5
# [ABAUD] serial line speed of the TNC
# [BBAUD] serial line speed of the GPS connected through the splitter cable
# If you remove these variables, PinPoin will not be able to set the parameters you configured in the Options menu
#
# GPS Passthrough by default every 3 seconds
[ESCAPE]
[PAUSE]
[ESCAPE]
[PAUSE]
[ESCAPE]
[PAUSE]
[PAUSE]
GRELAYBITS 3
GRELAYRATE 3
#
# Set up path
#
PATH1 [PATH1]
[PAUSE]
PATH2 [PATH2]
[PAUSE]
PATH3 [PATH3]
[PAUSE]
#
# Do not beacon (handled by PinPoint), set up digi.
#
PPERIOD 0
MPPERIOD 0
WPERIOD 0
BPERIOD 0
SBEN FALSE
[PAUSE]
ALIAS1 [ALIAS1]
[PAUSE]
ALIAS2 [ALIAS2]
[PAUSE]
ALIAS3 [ALIAS3]
[PAUSE]
#
# A channel in TEXT mode, B channel in GPS mode, set call sign
#
AMODE TEXT
ABAUD [ABAUD]
[PAUSE]
BMODE GPS
BBAUD [BBAUD]
[PAUSE]
PKTICOM TRUE
PKTOCOM FALSE
[PAUSE]
DIGIID TRUE
MYCALL [MYCALL]
#
# Exit config mode
#
QUIT