Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## org.ka2ddo.yaac.ax25
Interface DuplicateCheckedAX25Listener

All Known Implementing Classes:
  KenwoodMessageListTableModel, KenwoodRadioViewPane

    public interface DuplicateCheckedAX25Listener

This interface defines a listener for decoded AX.25 frames, but indicates whether or not it is a duplicate frame.

Method Summary
`void` | `consumeAX25Frame(AX25Message msg, AX25Frame frame, Connector connector, boolean isDuplicate)` Called when a AX.25 frame is received.

Method Detail

### consumeAX25Frame

    void consumeAX25Frame(AX25Message msg,
                          AX25Frame frame,
                          Connector connector,
                          boolean isDuplicate)

  Called when a AX.25 frame is received.

  Parameters:
    `msg` - decoded APRS message if the AX.25 frame contains an APRS packet, or null if the frame is not a recognized protocol
    `frame` - received AX25Frame
    `connector` - the PortConnector over which the frame was received
    `isDuplicate` - boolean true if this is a duplicate message (possibly received over a different digipeater path)

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD