
   Completed the first stage of the IQmonitor Pro installation -
unpacked the IQmonitor_Pro.zip archive and got the base directory
IQmonitor_Pro, which contains the basis of the program database,
StreamReader 1.2.4.109 and other files necessary for the program to work,
including the configs folder where you can easily save
ini files for each satellite - frequency range - frequency step in kHz.

   You need to edit the file in a text editor
IQmonitor_Pro.ini, in which to enter your data:

1. In the [USALS] section, set your coordinates with an accuracy of 1-3 digits
   after the decimal point (. point);

Lattitude = 50.62
Longitude = 30.51

   the diameter of your antenna (or the size of the minor axis of the ellipse) and the type of LNB,
   as well as the antenna aperture in centimeters;
                                                                                                                                                          
Antenna = 1.05m Inverto Black Ultra
Apertura = 105

   if your antenna is mounted on a moto suspension, indicate the number
   motor steps to rotate it by 1°;
 
Steps / degree = 64

2. In the [PARSER] section it is necessary to register the paths to the exe-files
   stream analyzers and viewers using the following example:

TSRLite = D: \ TSReaderLite \ TSReaderLite.exe
TSR = C: / Program Files (x86) /COOL.STF/TSReader/TSReader.exe
TrEdit = C: \ TransEdit \ TransEdit.exe
4T2ContentAnalyser = D: \ Program Files (x86) \ Abc \ 4T2 Content Analyzer \ ABC4T2ContentAnalyser.exe
MPC-BE = C: / MPC-BE x64 / mpc-be64.exe
VLC = C: / Program Files (x86) /VideoLAN/Vlc/vlc.exe

3. Programs TSReaderLite and ABC4T2ContentAnalyser need to be configured
   to read the transport stream file ...\ IQmonitor_Pro \ TS.ts,
   and the rest - to listen on port 2103 via UDP protocol

4. In the [CALIBRATION] section, you can set the noise factor of your
   receiving setting in dB or leave the same as the author's:

LNB_NF = 0.74

   After making the changes, save the IQmonitor_Pro.ini file

   Now unpack the archive IQmonitor_Pro_xxxx.zip (where xxxx is the number
version of the program) and copy IQmonitor_Pro.exe to the IQmonitor_Pro folder
This completes the installation of the program, you can run it and
enjoy the wide possibilities that will open before you

   Having mastered this or that function of the program, share your results
in the topic https://www.satellitescommunity.de/forum/index.php?thread/1565-iqmonitor-tool/&postID=44542#post44542
 
   ATTENTION ! Publication of your materials on the forum www.satellitescommunity.de
is a NECESSARY condition for obtaining a personalized key to the IQmonitor_Pro program

   When you decide that you have mastered all the basic functions of the program and confirmed
these are your publications on the forum, you lead the best in the topic (according to your
opinion) the result of using the IQmonitor_Pro program and submit an application
to receive a personalized key to the program, which opens Advanced functions
   When the moderator decides that you have sufficient command of the program,
the file IQmonitor_Pro.key will be sent to you through the system of private messages, which
you just need to put it in the IQmonitor_Pro folder.

   Good luck! Yours faithfully Yuri Filatov aka wanderer