# MOTOTRBO Customer Programming Software

### Table of Contents

1. Introduction

2. What's new in this release

3. Requirements

4. Installation, Removal

5. Legal notice

6. Motorola Solutions Publically Available Software Legal Notices Document

### 1. Introduction

Welcome to the MOTOTRBO Customer Programming Software (CPS) for the XiRP8268, XiRP8260, XiRP8208, XiRP8200, XiRM8260, XiRM8268 and XiRM8220 radios.

### 2. What's new in this release

Version | Notes
6.5 (Build 289) | Support for Digital Telephone Patch feature. Support for One-Touch Telemetry Revert feature. Support for Enhanced Channel Access feature in Conventional Mode. Support for Power Alert Disable and Text Message Alert features.
6.0 (Build 244) | Support for IP Remote Repeater Programming feature. Support for Enhanced GPS feature. Support for Transmit Interrupt feature in IP Site Connect and Capacity Plus Modes. Support for converting from MOTOTRBO Conventional Radios to 3600 Trunking Capable Radios. Support for Analog Voting feature for MTR3000 repeaters.
5.6 (Build 223) | Support for extended ramp-up time for 3600 Trunking Capable Radios. Support for Dynamic Mixed Mode feature for MTR3000 repeaters. Support for 800/900 Bands for MTR3000 repeaters. Support for Transmit Interrupt feature in Conventional Mode for MTR3000 repeaters.
5.5 (Build 213) | Support for converting from 3600 Trunking Capable Radios to MOTOTRBO Conventional Radios, 350MHz, Canada Full Frequency Range and Talk Group Scan List.
5.2 (Build 189) | Support for Dynamic Mixed Mode feature.
5.1 (Build 179) | Support for Microsoft® Windows® 7 Home Premium and Professional Editions.
5.0 (Build 177) | Support for Transmit Interrupt feature. Support for Quik Call II feature. Support for Home Revert feature. Support for up to 32 MDC systems. Support for 800/900 Bands models. Support for T3000A UHF Range 1 and Range 2 model. Support for 3600 Trunking Capable Radios
4.6 (Build 163) | Support for purchasing radio features.
4.5 (Build 144) | Support for Capacity Plus feature.
4.0 (Build 112) | Support for IP Site Connect feature. Support for Enhanced Privacy feature. Support for up to 1000 Channels with memory utilization information. Support for Table View configuration of Channels, Calls and Signaling Systems. Drag and drop feature enhanced to support General Settings, Accessories, Buttons, Text Messages, Telemetry, Menu, Privacy and Network. Support for cloning multiple (4) devices from a single archive simultaneously.
3.6 (Build 97) | Support for In Call Criteria and Digital Microphone Gain configuration. Fix for the error message issue when there is no audio device available. Fix for non-GPS radio cloning issue using the codeplug version less than 03.00.08 archive files.
3.5 (Build 88) | Support for GPS Revert feature. Support for UHF Band 2 models. Support to preserve sorted items. Support for disabling warning messages. Support for Microsoft® Windows® Vista Home Premium and Business Editions.
3.0 (Build 80) | Support for additional UHF/VHF high/low power models. Support for searching the controls on the configuration view. Support for getting to the selected channel from the list of channels on the zone configuration view using “Go to” feature. Configuration of the GPIO Pins has been changed from logical pin numbers to actual physical pin numbers. Opening old archives will result in reordering of the logical pin numbers to the physical pin numbers (actual operation will not be affected). Refer to online help for the pin number mapping.
2.0 (Build 67) | Support for VHF high power models.
1.0 (Build 59) | Support for the MOTOTRBO UHF radios. Drag and drop support between models. Support for renaming channels, systems, calls and lists. Support for multiple selection configuration. For example, create several Digital Channels and select them all in the tree view and set the Slot of all the Digital Channels to the same value at once. Support for custom views and undo/redo. Support for loading language packs in the radio to navigate radio menu and features in different languages. Support for firmware and codeplug upgrade using the device update feature.

### 3. Requirements

Operating System |  |
Microsoft® Windows® 7 Home Premium Edition Microsoft® Windows® 7 Professional Edition Microsoft® Windows® Vista Home Premium Edition Microsoft® Windows® Vista Business Edition Microsoft® Windows® XP Home/Professional Edition with SP2 or SP3 and Windows Installer 3.1 |  |  |
Hardware Recommendations
· The application takes approximately 400 MB of free disk space on your PC. However, more space would be required to save archive files of your radios and device update packages. Each archive file or device update package varies in size depending on the features of the radio.
· For processor speed and RAM, the recommendations given by Microsoft for the release of the operating system that you are using should be sufficient.
· A USB port.
· A CD-ROM drive.
Software Recommendations
· Running multiple instances of the CPS application is not recommended. |  |  |

### 4. Installation, Removal

Installation
You need to have Administrator rights on the target PC in order to install the software. Follow the steps below for the CD-ROM version: · Before inserting the CD-ROM, disable any virus scanning or firewall software, which may interfere with the installation process. · Insert the CD-ROM containing the installation into the CD-ROM drive. · If the installation application doesn't start within 30 seconds, the auto-run feature for CD-ROMs for you operating system is likely disabled. Browse to your CD-ROM and run the autorun.exe program. For example, if the E:\ drive is the CD-ROM, run E:\autorun.exe. Follow the steps below for the software package version: · Before starting the setup.exe program, disable any virus scanning or firewall software, which may interfere with the installation process. · Unzip the CPS package to a directory of a local disk. · Browse to this directory and run the setup.exe program. If a previous version of CPS has already been installed, you will be given the option to “Repair” or “Remove”. If you are upgrading the CPS, then remove the previous version and start the installation process again. If you are re-installing the CPS, then choose the repair option. Note: 1. Microsoft Visual C++ 2005 Redistributable, which is installed as part of CPS installation, will not be re-installed thru the Repair option. 2. During re-install, settings for preferences and dealer information will be reset to their default values. You will need to check these settings after the new version has been installed and make changes as necessary.
Removal
From the Start button on the task bar of your operating system, select Settings > Control Panel. Select the Add/Remove Programs option within the control panel. Select the MOTOTRBO Customer Programming Software item in the "Currently installed programs" box and click the remove button.

### 5. Legal notice

Motorola Solutions and MOTOTRBO are registered trademarks of Motorola Solutions, Inc.

Microsoft® and Windows® are registered trademarks of Microsoft Inc.

### 6. Motorola Solutions Publically Available Software Legal Notices Document

###