A "startpb" script has been added for Portable Predict Plus that
performs the duties of setting the AX.25 parameters for full-duplex
communications, starting pb, and running pbctrl.  Once ended (by
hitting 'Q'), "stoppb" is called, and the AX.25 port is returned
to half-duplex mode.

73, de John, KD2BD

