F8 - ERROR CONDITIONS                                                                                                                                               KEY "BEEPS"      - Pressing an invalid key will cause a short "beep".                              Press <F1> for a list of available commands.                                                                                                 CONNECTION ERROR - The program has read all-blank information from                                 the module, possibly due to a faulty module or                                  poor connection.                                                                                                                             PROGRAMMING      - The information read back during the automatic               FAILED             verification step does not agree with the setup,                                possibly due to a faulty module or poor connection.                                                                                          INCORRECT        - The Programming Interface hardware is either of the          PROGRAMMER or      incorrect type, or is not connected to the computer          PROGRAMMER NOT     printer port. If a port switch is used, it may be in         CONNECTED          the wrong position.                                                                                                                          NO POWER TO      - The Programming Interface is connected, but power is         PROGRAMMER         not applied.                                                                    (Applies only to those with power-sense circuitry)                                                                                           FILE NOT FOUND   - The required setup file was not found. Please check                             correct entry of name or press <F9> to list the                                 directory of setup files.                                                                                                                    NO COMMAND.COM   - The <F9> Directory screen requires that the                                     COMMAND.COM  DOS program be available via the PATH                              or COMSPEC settings in the DOS environment.                                     Refer to the MS-DOS or PC-DOS manual for information.                                                                                    